# DIGITAL TCP/IP Services for OpenVMS
Management Command Reference

Previous | Contents

### E

- ENABLE SERVICE command
- Error logging
  - See Event logging
- ETC.BOOTPTAB file
  - CONVERT/VMS BOOTP command
- /etc/hosts
  - CONVERT/ULTRIX HOST command
  - CONVERT/VMS HOST command
- /etc/mount command
- /etc/networks
  - CONVERT/ULTRIX NETWORK
  - CONVERT/VMS NETWORK
- Ethernet
  - address
    - mapping to IP #1
    - mapping to IP #2
  - allocating buffers
  - controller
    - identifying with SET INTERFACE command
    - zeroing counters
- Ethernet controller
  - See Network device
- Event logging
  - setting for all services
- eXchange IDentification
  - See XID
- EXIT command
- EXPORT command
- Export Database
  - adding directory names in the Export Database
  - CREATE EXPORT command
  - deleting directory names from the Export Database
  - SHOW EXPORT command

### F

- FDDI
  - address
    - mapping to IP #1
    - mapping to IP #2
  - allocating buffers
  - controller
    - identifying with SET INTERFACE command
    - zeroing counters
- FDDI controller
  - See Network device
- Fiber Distributed Data Interface
  - See FDDI
- File
  - multiple names
    - on command lines
  - names
    - using lowercase
    - using quotation marks
    - using wildcards
- File identification
  - See FID
- File system
  - See NFS
- File Transfer Protocol
  - See FTP
- Files-11 On-Disk Structure
  - See ODS-2
- FTP
  - disabling
  - enabling
    - upon system startup
  - monitoring

### G

- GENERATE MAP command

### H

- Hardware
  - See Network device
- Hardware device
  - See Network device
- HELP command
- Host
  - entry in Hosts Database
  - name-to-address lookups
    - See Lookups
- Host address
  - defining #1
  - defining #2
  - displaying
  - how to specify
- Host name
  - how to specify
- Hosts Database
  - cluster alias
    - specifying
  - CONVERT/ULTRIX HOST command
  - CONVERT/VMS HOST command
  - SHOW HOST command

### I

- ICMP
  - counters
    - resetting
  - ECHO packets
    - for testing #1
    - for testing #2
  - parameters
    - setting #1
    - setting #2
  - starting #1
  - starting #2
- IMPORT command
- Interface
  - See Internet interface
- Internet
  - device driver #1
  - device driver #2
  - device driver #3
  - device driver #4
- Internet Control Message Protocol
  - See ICMP
- Internet interface
  - cluster broadcast mask
    - defining
  - cluster network mask
    - defining
  - defining #1
  - defining #2
  - defining broadcast address for
  - displaying
  - new device
    - defining
    - deleting
    - displaying
  - pseudo-interface
    - defining #1
    - defining #2
    - displaying
  - testing
    - SET INTERFACE /LOOPBACK command
- Internet Protocol
  - See IP
- Interprocess communication
  - See APIs
- IP
  - address
    - mapping to Ethernet #1
    - mapping to Ethernet #2
  - counters
    - resetting
  - parameters
    - setting #1
    - setting #2
  - starting #1
  - starting #2

### L

- LIST COMMUNICATION_CONTROLLER command
- Load balancing
  - See BIND Server
- Logging
  - See Event logging
- Lookups
  - by BIND resolver #1
  - by BIND resolver #2
  - by BIND resolver #3
  - in Hosts database #1
  - in Hosts database #2
  - in Hosts database #3
  - in Hosts database #4
  - in Hosts database #5
  - in Hosts database #6
  - in Hosts database #7
  - local
  - using BIND Resolver
  - using Hosts Database
- LOOP command
- /LOOPBACK qualifier
  - testing internet interfaces
- LPD
  - ADD PROXY command #1
  - ADD PROXY command #2
  - CREATE PROXY command
  - disabling
  - enabling
    - upon system startup
  - monitoring
  - registering clients #1
  - registering clients #2

### M

- Mail
  - See SMTP
- Mail exchanger
  - See MX Database
  - See SMTP
- Mail Exchanger Database
  - See MX Database
- MAP command
- Mapping
  - file system to NFS Server
    - See MAP command
    - See NFS
  - name to address
    - See Lookups
- Master File Directory
  - See MFD
- Memory buffer
  - See MBUF
- MFD
  - specifying
- MOUNT
  - enabling
    - upon system startup
- MOUNT command
- MOUNT command (DCL)
  - similar to SET CONFIGURATION
- Mount point
  - dismounting
  - specifying #1
  - specifying #2
- Mounting
  - DISMOUNT command
  - displaying mounted file systems
    - SHOW MOUNT command
  - mount point
    - specifying
  - remote directories
    - MOUNT command
- Multiple
  - files
    - how to specify
  - hosts
    - how to specify
  - options
    - how to specify
- MX
  - See MX Database
  - See SMTP
- MX Database
  - routing mail
    - SET MX_RECORD command
    - SHOW MX_RECORD command

### N

- Name service
  - See DNS
- Name-to-address lookups
  - See Lookups
- Network
  - name-address lookups
    - SET NETWORK command
    - SHOW NETWORK command
- Network management
  - remote
    - See SNMP
  - See individual topics
- Network print services
  - See Printing
- Networks database
  - adding entries
- Networks Database
  - CONVERT/ULTRIX NETWORK
  - CONVERT/VMS NETWORK
  - displaying entries
- NFS
  - Client
    - ADD PROXY command #1
    - ADD PROXY command #2
    - CREATE PROXY command
    - DISMOUNT command
    - enabling
      - upon system startup
- MOUNT command
- mount point
  - dismounting
  - specifying

- registering clients #1
- registering clients #2
- SHOW MOUNT command
- PC-NFS
  - See PC-NFS
- Server
  - ADD PROXY command #1
  - ADD PROXY command #2
  - adding directory names in the Export Database
  - ANALYZE CONTAINER command
  - container directory
    - displaying
- copying container directory files to OpenVMS files
- copying OpenVMS files to container directory files
- counters
  - displaying
  - resetting
- CREATE DIRECTORY command
- CREATE EXPORT command
- CREATE PROXY command
- DELETE CONTAINER command
- deleting directory names from the Export Database
- directories
  - creating
- DIRECTORY command
- enabling
  - upon system startup
- EXPORT command
- GENERATE MAP command
- IMPORT command
- links
  - creating
  - deleting #1
  - deleting #2
- making files available for mounting #1
- making files available for mounting #2
- making files available for mounting #3
- making files unavailable
- MAP command
- mapping
  - SHOW MAP command
- mapping file systems
  - SET CONFIGURATION MAP command
  - SHOW CONFIGURATION MAP command
  - UNMAP command
- NFS clients
  - making files unavailable to
- parameters
  - displaying
  - setting
- performance
  - monitoring
  - resetting counters
  - setting parameters
- registering clients #1
- registering clients #2
- REMOVE DIRECTORY command
- REMOVE FILE command
- REMOVE PROXY command
- restarting
- SET CONFIGURATION MAP command
- SET CONFIGURATION NOMAP command
- SET NFS_SERVER command
- SHOW EXPORT command
- SHOW MAP command
- SHOW NFS_SERVER command
- SHOW PROXY command
- showing clients
- UNIX-style file system
  - creating
- UNMAP command
- unmapping file systems
  - SET CONFIGURATION NOMAP command
- unregistering clients
- ZERO NFS_SERVER command
- Nonpaged pool
  - affected by device sockets
  - affected by free buffers #1
  - affected by free buffers #2
  - affected by IRPs
  - affected by non-UCX buffers

  ### O

  - ONC
    - See RPC
  - Online help
    - HELP command
    - See Help
  - Open Network Computing (ONC)
    - See RPC
  - OpenVMS Cluster
    - broadcast mask
      - defining
    - /CLUSTER_TIMER qualifier
    - copying configuration to another node
    - displaying internet interface information
    - network mask
      - defining
    - SMTP queues

  Previous | Next | Contents