# DIGITAL TCP/IP Services for OpenVMS
Installation and Configuration

Previous | Contents

After you configure the server components, as in the preceding example script, press Return to go to the main Configuration menu. Enter option 4, Optional Components.

## 3.2.2 Configuring the Optional Components

You may need to configure optional UCX components if you plan to do one or more of the following:

- Run PATHWORKS or DECnet over TCP/IP.
- Run or develop applications that use the Stanford Research Institute's (SRI) QIO application programming interface (API).
- Allow guest users to log into the system at various locations.

Configure the optional components as follows:

1. Invoke the command procedure:

       $ @SYS$MANAGER:UCX$CONFIG

   The main Configuration menu displays:

       DIGITAL TCP/IP Services for OpenVMS Configuration Menu

       Configuration options:

               1 - Core environment
               2 - Client components
               3 - Server components
               4 - Optional components

               5 - Shutdown TCP/IP Services for OpenVMS
               6 - Startup TCP/IP Services for OpenVMS
               7 - Run tests

               A - Configure options 1 - 3
             [E] - Exit configuration procedure

       Enter configuration option:

2. Enter option 4. The Optional Components menu displays:

       DIGITAL TCP/IP Services for OpenVMS Optional Components Menu

       Configuration options:

               1 - Configure PWIP Driver
               2 - Configure SRI QIO Interface
               3 - Set up Anonymous FTP Account and Directories
             [E] - Exit menu

3. Enter the options that are appropriate for your system: the PWIP driver, the SRI QIO interface, or Anonymous FTP accounts or directories:
   - If you want to run PATHWORKS or DECnet over TCP/IP, configure the PWIP driver by entering option 1.
   - If you run or develop applications that use the SRI QIO API, enter option 2. Alternatively, you can load the interface by issuing the following command:

         $ @SYS$MANAGER:UCX$LOAD_INETDRIVER.COM

   - If you want to allow guest users to log into the system, set up an Anonymous FTP Account and Directories by entering option 3. Make sure you obtain the necessary user information code (UIC; see Section 1.2.7) and determine guest user privileges.

   # 3.3 Using UCX$CONFIG Option Commands

   If you are an experienced user of the UCX product, you may want to bypass the configuration menus to enable or disable functionality, as follows:

   1. Log into the SYSTEM account.
   2. Invoke the command procedure and include the appropriate options in the command line:
   @SYS$MANAGER:UCX$CONFIG
   - ALL
   - CLIENT
   - SERVER
   - MINIMUM
   - WORKSTATION
   - ENABLE
   - DISABLE

   or
   @SYS$MANAGER:UCX$CONFIG

   - ALL
   - CLIENT
   - SERVER
   - WORKSTATION
   - MINIMUM
   - ENABLE
   - DISABLE
   CLUSTER

   For example, the following command enables the client components for the entire cluster:

       $ @SYS$MANAGER:UCX$CONFIG CLIENT ENABLE CLUSTER

   The available options are as follows:

   Parameter | Description
   --- | ---
   ALL | Configures the core environment and all client and server components.
   CLIENT | Configures all client components and related software.
   SERVER | Configures all server components and related software.
   WORKSTATION | Configures the BIND resolver, the domain, dynamic routing, Internet interfaces, time zone, remote login, remote shell, remote executive, FTP client, FTP server, TELNET client, TELNET server, and SMTP.
   MINIMUM | Configures the domain, Internet interfaces, remote login, FTP client, FTP server, TELNET client, and TELNET server.
   ENABLE | Enables all the configured components.
   DISABLE | Disables all the configured components.
   CLUSTER | Configures all selected components clusterwide (except for the BIND server and SMTP, which you cannot configure clusterwide). If you configure at least one cluster interface, the procedure automatically enables IP forwarding.

   > Note

   > The procedure implements two levels of enabling and disabling: clusterwide and single node (except for the BIND server and SMTP, which are configured and enabled as node-specific only).

   # 3.4 Starting UCX

   You must start UCX after you configure the standard software and optional components, but before you run tests or customize the UCX environment.

   Start UCX on your system as follows:

   1. Access the main Configuration menu by entering the following command:

          $ @SYS$MANAGER:UCX$CONFIG

   2. Enter option 6 to start UCX.

   # 3.5 Verifying the Configuration

   You can verify the UCX configuration by running the installation verification procedure (IVP).

   You should run the IVP if the following apply:

   - If you loaded the Product Authorization Key (PAK), and you want to verify that the lower-layer software and the Portmapper service are installed correctly.
   - If you did not load the PAK, but you want to verify that UCX is installed correctly for DECwindows to display UCX applications.
   - To transfer device socket packets that continuously vary in size, between a sender and a receiver.
   - To test the Portmapper service with a pair of client/server programs. The IVP reports the time it took to run the test to SYS$OUTPUT.

   Before you run the IVP, make sure the UCX software is started and you have SYSPRV, OPER, NETMBX, and TMPMBX privileges. (You use the SETPRV command to set the privileges.)

   Run the IVP as follows:

   1. Invoke the command procedure:

          $ @SYS$MANAGER:UCX$CONFIG

   2. Enter option 7. If the IVP does not complete successfully, the procedure displays error messages. All IVP errors are fatal and use the same format as system messages. For example:

          %UCX-E-IDENT, explanation of error.

      Table 3-2 lists some common problems that cause IVP error messages. If the recommended action does not correct the problem, contact your DIGITAL support representative.

      Table 3-2 Troubleshooting IVP Errors
      Problem | Corrective Action
      --- | ---
      Network configuration is incorrect. | Shut down the UCX software and rerun the configuration procedure.
      Startup fails. | Check the SYSGEN parameters in the MODPARAMS.DAT file and increase them if necessary. Shut down and restart UCX.
      The installation kit is defective. | Request a replacement kit.
      The IVP fails because the PAK is missing. | Register a DIGITAL TCP/IP Services for OpenVMS PAK.

   3. To run the IVP any time after exiting the configuration procedure, invoke the IVP command procedure as follows:

          $ @SYS$TEST:UCX$IVP

   4. To activate the new configuration, reboot your system.

   # 3.6 Additional Configuration Tasks

   After you run the configuration procedure and enable the functionality and components appropriate for your network, you need to complete additional configuration tasks to enable access to UCX applications. UCX provides a management command interface and logical names you can use to modify or customize the software for your environment.

   The additional configuration tasks include:

   - Populating databases
   - Setting up user accounts
   - Setting up communication and NFS proxies
   - Defining print queues
   - Setting up, exporting, and maintaining file systems
   - Tuning the system for optimum performance

   For information about these and other configuration tasks, see the DIGITAL TCP/IP Services for OpenVMS Management guide.

   # 3.7 Automatically Starting and Stopping UCX

   To start the UCX software automatically when the system starts up, edit the SYS$MANAGER:SYSTARTUP_VMS.COM file and include the following command line after the command line that starts the procedure:

       @SYS$MANAGER:UCX$STARTUP

   To stop UCX automatically when the system shuts down, add the following command line to the SYS$MANAGER:SYSHUTDOWN.COM file:

       @SYS$MANAGER:UCX$SHUTDOWN

   # 3.8 Automatically Starting UCX Services

   For the UCX services to start after you log into your OpenVMS account, the OpenVMS systemwide login procedure (typically SYS$MANAGER:SYLOGIN.COM) must be world-readable and world-executable.

   To display the current privileges, issue:

       $ DIRECTORY SYS$MANAGER:SYLOGIN.COM /PROTECTION

   If the protections are not world read and edit (W:RE), issue:

       $ SET PROTECTION=(W:RE) SYS$MANAGER:SYLOGIN.COM

   # 3.9 Specifying UCX as the Transport for DECwindows Applications

   To enable the UCX software as the transport interface for DECwindows applications, add the following line to the SYS$MANAGER:DECW$PRIVATE_SERVER_SETUP.COM command procedure:

       $ DECW$SERVER_TRANSPORTS == "DECNET,LOCAL,TCPIP"

   Then restart DECwindows by entering the following command:

       $ @SYS$STARTUP:DECW$STARTUP RESTART

   If DECnet or DECnet-Plus runs on the same system, start it.

   To display DECwindows applications from a DECwindows client (remote host) to a DECwindows server (your workstation), proceed as follows:

   1. Set up security on the remote host.
   2. Add the remote client to the local UCX hosts database.
   3. Edit the SYS$MANAGER:DECW$PRIVATE_SERVER_SETUP.COM command procedure by adding the following line:

          $ DECW$SERVER_TRANSPORTS == "DECNET,LOCAL,TCPIP"

   4. Set the display for the applications to the remote host:

          $ SET DISPLAY/CREATE/NODE=remote_host/TRANSPORT=TCPIP

   # Appendix A
   Installed Files

   The installation procedure installs all the UCX distribution files appropriate for your operating system.

   If you are upgrading from a previous version of UCX, the procedure renames the configuration database in SYS$COMMON:[SYSEXE] from UCX$CONFIGURATION.DAT to UCX$CONFIGURATION.OLD.

   # A.1 Installed UCX Files

   Table A-1 outlines the UCX files installed on your system.

   Table A-1 UCX Files
   File Name / Logical Name | Description
   --- | ---
   SYS$COMMON:[SYS$LDR] / SYS$LOADABLE_IMAGES: |
   UCX$BGDRIVER.EXE | Internet device driver
   UCX$DNFSDRIVER_V5.EXE+ | OpenVMS Version 5 NFS client driver
   UCX$DNFSDRIVER_V6.EXE+ | OpenVMS Version 6 NFS client driver
   UCX$DNFSDRIVER.EXE | AXP image
   UCX$INETDRIVER.EXE | SRI QIO driver
   UCX$INTERNET_SERVICES.EXE+ | Internet software
   UCX$INTERNET_SERVICES_V6.EXE+ | Internet software
   UCX$TNDRIVER.EXE | TELNET and remote login drivers
   SYS$COMMON:[SYSEXE] / SYS$SYSTEM: |
   UCX$CONVERT.FDL | File definition used by UCX$CONVERT.COM
   UCX$CONVERT.COM | Procedure for converting files to STREAM_LF
   UCX$BIND_SERVER.EXE | BIND server
   UCX$BIND_SERVER_XFER.EXE | BIND server's zone transfer
   UCX$BOOTP.EXE | Remote boot server
   UCX$ENCODE.COM | Procedure to execute UUencode program
   UCX$EXE.ADF | Attributes file for NFS client
   UCX$DECODE.COM | Procedure to execute UUdecode program
   UCX$DNFSMOUNT_V5.EXE | VAX image
   UCX$DNFSMOUNT_V6.EXE | VAX image
   UCX$DNFSDISMOUNT_V5.EXE | VAX image
   UCX$DNFSDISMOUNT_V6.EXE | VAX image
   UCX$DNFSACP_V5.EXE | VAX image
   UCX$DNFSACP_V6.EXE | VAX image
   UCX$ESNMP_SERVER.EXE | eSNMP server
   UCX$FINGER.EXE | Finger client
   UCX$FINGER_SERVER.EXE | Finger server
   UCX$FTP.EXE | FTP client
   UCX$FTPC.EXE | FTP server
   UCX$FTPD.EXE | FTP control command server (daemon)
   UCX$FTPSERVER.COM | Procedure that starts an FTP child process
   UCX$HLB.ADF | Attributes file for NFS client
   UCX$HR_MIB.EXE | SNMP Host Resources MIB
   UCX$INETACP.EXE | Network ancillary control process (NETACP) for the Internet device driver
   UCX$INETACP.STB | Global symbol definitions for UCX$INETACP.EXE
   UCX$INETDRIVER.STB | Global symbol definitions for the Internet device driver
   UCX$INTERNET_SERVICES_V6.STB+ | Global symbol definitions for UCX$INTERNET_SERVICES_V6.EXE
   UCX$INTERNET_SERVICES_V6_SEC.STB+ | Global symbol definitions for UCX$INTERNET_SERVICES_V6_SEC.EXE
   UCX$INTERNET_SERVICES.STB | Global symbol definitions for UCX$INTERNET_SERVICES.EXE
   UCX$INTERNET_SERVICES_SEC.STB | Global symbol definitions for UCX$INTERNET_SERVICES_SEC.EXE
   UCX$INET_ROUTING.EXE | Dynamic routing
   UCX$INET_ROUTING.STB | Global symbol definitions for UCX$INET_ROUTING.EXE
   UCX$LPD_RCV.EXE | Print receiver
   UCX$LPD_SMB.EXE | Print symbiont
   UCX$LPRM.EXE | LPRM command
   UCX$LPRSETUP.EXE | Setup utility for network printing
   UCX$LPQ.EXE | LPQ command
   UCX$METRIC.EXE | Metric server
   UCX$METRIC_VIEW.EXE | Metricview utility
   UCX$MIBCOMP.EXE | SNMP MIB compiler
   UCX$MLB.ADF | Attributes file for NFS client
   UCX$MOSY.EXE | MIB compiler images
   UCX$NET_GLOBALS.STB | Global symbol definitions for UCX data structures
   UCX$NSLOOKUP.EXE | NSLOOKUP utility
   UCX$NTPD.EXE | NTP service
   UCX$OBJ.ADF | Attributes file for NFS client
   UCX$OLB.ADF | Attributes file for NFS client
   UCX$OS_MIBS.EXE | MIB-II subagent image
   UCX$PCNFSD.EXE | PC-NFS server (daemon)
   UCX$POP_SERVER.EXE | POP server image
   UCX$PING.EXE | PING command image
   UCX$PORTMAPPER.EXE | Program that maps processes to ports
   UCX$RLOGIN.EXE | Remote login client
   UCX$RPCGEN.EXE | Portmapper image
   UCX$RPCINFO.EXE | SHOW PORTMAPPER command
   UCX$RSH.EXE | Remote shell
   UCX$SERVER_NFS.EXE | NFS server (daemon)
   UCX$SMTP_RECEIVER.EXE | SMTP receiver
   UCX$SMTP_SYMBIONT.EXE | SMTP symbiont
   UCX$SNMP_AGENT.EXE | SNMP agent
   UCX$SNMPI.EXE | MIB compiler images
   UCX$SNMP_REQUEST.EXE | MIB browser
   UCX$STB.ADF | Attributes file for NFS client
   UCX$TELNET.EXE | TELNET client
   UCX$TELNETSYM.EXE | TELNET print symbiont
   UCX$TFTP.EXE | TFTP server (daemon)
   UCX$TLB.ADF | Attributes file for NFS client
   UCX$TNDRIVER.STB | Global symbol definitions for UCX$TNDRIVER.EXE
   UCX$RCP.EXE | RCP image
   UCX$RMT.EXE | RMT/RCD server
   UCX$UCP.EXE | UCX Management Control Program (UCP)
   UCX$UUENCODE.EXE | UUencode program image
   UCX$UUDECODE.EXE | UUdecode program image
   UCX$VERSIONS.EXE | Image for the SHOW VERSION command
   SYS$COMMON:[SYSLIB] / SYS$LIBRARY: |
   UCX$ACCESS_SHR.EXE | Database access routines
   UCX$CFS_SHR.EXE | Container file system runtime library
   UCX$ESNMP_SHR.EXE | Sharable image version of routines in UCX$SNMP:*.OLB
   UCX$INETDEF.ADA | Internet Ada definitions file
   UCX$INETDEF.BAS | Internet BASIC definitions file
   UCX$INETDEF.FOR | Internet FORTRAN definitions file
   UCX$INETDEF.H | Internet C definitions file
   UCX$INETDEF.MAR | Internet MACRO definitions file
   UCX$INETDEF.PAS | Internet Pascal definitions file
   UCX$INETDEF.PLI | Internet PL/1 definitions file
   UCX$INETDEF.R32 | Internet BLISS definitions file
   UCX$IPC_SHR.EXE | IPC runtime library
   UCX$IPC.OLB | IPC object library
   UCX$LPD_SHR.EXE | Shared library for printing processes
   UCX$RPCXDR.H | Sun RPC header file
   UCX$RPCXDR_SHR.EXE | Sun RPC routines library
   UCX$SDA.EXE | SDA extensions
   UCX$SMTP_MAILSHR.EXE | SMTP shared library
   UCX$SMTP_PARSESHR.EXE | SMTP parsing routines
   SYS$COMMON:[UCX$LIB.RPC] / SYS$LIBRARY: |
   UCX$RPCXDR.OLB | Library file for Portmapper service
   SYS$COMMON:[UCX$LIB.SNMP] / SYS$LIBRARY: |
   UCX$ESNMP.OLB | Library file for creating SNMP subagents
   SYS$COMMON:[SYSHLP] / SYS$HELP: |
   UCX042.RELEASE_NOTES | Release notes
   UCX$FTP_HELP.HLB | FTP online help
   UCX$TELNET_HELP.HLB | TELNET online help
   UCX$NSLOOKUP_HELP.HLB | NSLOOKUP online help
   UCX$UCP_HELP.HLB | Online help for the management commands
   UCX$VMS_FILES.DOC | Online information about file restrictions for UNIX users of NFS server
   SYS$COMMON:[SYSHLP.EXAMPLES.UCX] / UCX$EXAMPLES: |
   BUILD_UCX_SECURITY_DRIVER.COM | Sample file to build the security driver
   TN3270DEF.MAR | For IBM 3270TE; translation table template that you edit to modify the translation tables
   TRACEROUTE.EXE | Traceroute facility
   UCX$CHESS_SUBAGENT.EXE | Linker image
   UCX$INTERNET_SERVICES_V6_SEC.EXE+ | Internet software with security for OpenVMS Version 6
   UCX$INTERNET_SERVICES_V5_SEC.EXE | Internet software with security for OpenVMS Version 5
   UCX$IOCTL_ROUTINE.C | C Programming example
   UCX$NFSSETUP.COM | NFS setup procedure
   UCX_SECURITY_DRIVER.MAR | MACRO security driver source sample
   UCX$TCP_CLIENT_IPC.C | C Programming example
   UCX$TCP_CLIENT_QIO.C | C Programming example
   UCX$TCP_CLIENT_QIO.MAR | C Programming example
   UCX$TCP_SERVER_IPC.C | C Programming example
   UCX$TCP_SERVER_IPC_AUXS.C | C programming example
   UCX$TCP_SERVER_QIO.C | C Programming example
   UCX$TCP_SERVER_QIO.MAR | MACRO Programming example
   UCX$TCP_SERVER_QIO_AUXS.C | C programming example
   UCX$TCP_SERVER_QIO_AUXS.2ND.C | C programming example
   UCX$TCP_SOCKET_QIO.3RD.C | C programming example
   UCX$TCP_SOCKET_QIO_3RD.H | Data and structure definitions that make up the exterior interface to UCX$TCP_SOCKET_QIO_3RD.C
   UCX$TRACE.EXE | Protocol trace facility
   UCX$TRACE_HAS_MOVED.EXE | Trace facility
   UCX$UDP_CLIENT_IPC.C | C programming example
   UCX$UDP_CLIENT_QIO.C | C programming example
   UCX$UDP_CLIENT_QIO.MAR | MACRO programming example
   UCX$UDP_SERVER_IPC.C | C programming example
   UCX$UDP_SERVER_QIO.C | C programming example
   UCX$UDP_SERVER_QIO.2ND.C | C programming example
   UCX$UDP_SERVER_QIO.3RD.C | C programming example
   UCX$UDP_SERVER_QIO.MAR | MACRO Programming example
   SYS$COMMON:[SYSHLP.EXAMPLES.UCX.SNMP] / UCX$EXAMPLES: |
   CHESS_METHOD.C | C programming example
   CHESS_MIB.C | C programming example
   CHESS_MIB.MY | Sample MIB chess game
   CHESS_SUBAGENT.OPT | Linker options file
   CHESS_TBL.C | C programming example
   CHESS_TBL.H | C header file
   SYS$COMMON:[SYSHLP.EXAMPLES.UCX.RPC] / UCX$EXAMPLES: |
   DIR_EXAMPLE.COM | DIR program procedure
   DIR.X | Remote OpenVMS directory listing protocol
   DIR_SERVER.C | C programming example
   MSG.X | Remote message printing protocol
   MSG_EXAMPLE.COM | Local version of PRINTMSG program procedure
   MSG_SERVER.C | C programming example
   PRINTMSG.C | C programming example
   RLS.C | C programming example
   RPRINTMSG.C | C programming example
   SYS$COMMON:[SYSMGR] / SYS$MANAGER: |
   SYS$NET_SERVICES_UCX.COM | DCL interface support procedure
   UCX$BINDSETUP.COM | BIND setup procedure
   UCX$BINDSETUP_HELP.TXT | Information about setting up the BIND server
   UCX$BIND_SHUTDOWN.COM | BIND server shutdown procedure
   UCX$BIND_STARTUP.COM | BIND server startup procedure
   UCX$BOOTP_SHUTDOWN.COM | Remote boot server shutdown procedure
   UCX$BOOTP_STARTUP.COM | Remote boot server startup procedure
   UCX$CALLBACKS.COM | Configuration procedure
   UCX$CONFIG.COM | Configuration procedure
   UCX$DNFS_SHUTDOWN.COM | NFS client shutdown procedure
   UCX$FINGER_SHUTDOWN.COM | Finger server shutdown procedure
   UCX$FINGER_SRVR_STARTUP.COM | Finger server startup procedure
   UCX$FTPD_SHUTDOWN.COM | FTP server shutdown procedure
   UCX$FTPD_STARTUP.COM | FTP server startup procedure
   UCX$INET_STARTUP.COM | Internet startup procedure
   UCX$INET_SHUTDOWN.COM | Internet shutdown procedure
   UCX$LOAD_INETDRIVER.COM | Command file that loads the SRI QIO programming interface
   UCX$LPD_RCV_STARTUP.COM | Print receiver startup procedure
   UCX$LPD_STARTUP.COM | Print server startup procedure
   UCX$LPD_SHUTDOWN.COM | Print server shutdown procedure
   UCX$METRIC_STARTUP.COM | Metric startup procedure
   UCX$METRIC_SHUTDOWN.COM | Metric shutdown procedure
   UCX$NFS_SERVER_STARTUP.COM | NFS server startup procedure
   UCX$NFS_SHUTDOWN.COM | NFS server shutdown procedure
   UCX$NFS_STARTUP.COM | NFS client startup procedure
   UCX$PCNFSD_SHUTDOWN.COM | PC-NFS server shutdown procedure
   UCX$PCNFSD_STARTUP.COM | PC-NFS server startup procedure
   UCX$PORTM_SHUTDOWN.COM | Portmapper shutdown procedure
   UCX$PORTM_STARTUP.COM | Portmapper startup procedure
   UCX$PRINTCAP.DAT | Printcap database
   UCX$REGISTER.COM | Command file that registers privileged UCX images for OpenVMS Version 6.2
   UCX$REMOTE_TTY_STARTUP.COM | TELNET and remote login server startup procedure
   UCX$REXECD_STARTUP.COM | Remote executive startup procedure
   UCX$RSHD_STARTUP.COM | Remote shell startup procedure
   UCX$SERVICE_SETUP.COM | UCX services set up procedure
   UCX$SHUTDOWN.COM | UCX shutdown procedure
   UCX$SMTP_STARTUP.COM | SMTP queue startup procedure
   UCX$SMTP_SHUTDOWN.COM | SMTP queue shutdown procedure
   UCX$SMTP_RECV_STARTUP.COM | SMTP receiver startup procedure
   UCX$SNMP_STARTUP.COM | SNMP startup procedure
   UCX$SNMP_SHUTDOWN.COM | SNMP shutdown procedure
   UCX$SNMPD_MIR.DAT | SNMP dictionary of MIB variables
   UCX$STARTUP.COM | UCX startup procedure
   UCX$SYMBOLS.COM | Configuration logical names
   UCX$TELNET_SHUTDOWN.COM | TELNET shutdown procedure
   UCX$TFTP_SHUTDOWN.COM | TFTP shutdown procedure
   UCX$TFTP_STARTUP.COM | TFTP startup procedure
   UCX$TIMEZONE.COM | Time zone procedure
   UCX$UCP_STARTUP.COM | Management control program startup
   SYS$COMMON:[SYSMSG] / SYS$MESSAGES: |
   UCX$MSG.EXE | UCX message file
   SYS$COMMON:[SYSTEST.UCX] / SYS$TEST: |
   UCX$INET_IVP.EXE | Auxiliary server IVP
   UCX$RPCIVP_CLIENT.EXE | RPC client routines IVP
   UCX$RPCIVP_SERVER.EXE | RPC server routines IVP
   UCX$SNMPIVP.EXE | SNMP IVP
   SYS$COMMON:[SYSTEST] |
   UCX$IVP.COM | UCX IVP procedure
   SYS$COMMON:[SYSUPD] |
   UCX$CLEANUP.COM | Procedure to remove UCX software from the OpenVMS system
   UCX$CLEANUP_HELPLIB.COM | Procedure to update the UCX help library

   +Specific to OpenVMS VAX

   # A.2 Installed UCX Files for PATHWORKS Systems

   Table A-2 lists and describes the files for PATHWORKS systems that are installed on your system.

   Table A-2 PATHWORKS Files
   File | Description
   --- | ---
   SYS$COMMON:[SYSLIB]PWIP$SDA.EXE | PATHWORKS extensions to SDA
   SYS$COMMON:[SYSEXE]UCX$PWIPACP.EXE | PATHWORKS IP ACP
   SYS$COMMON:[SYS$LDR]UCX$PWIPDRIVER.EXE | PATHWORKS IP driver
   SYS$COMMON:[SYSEXE]UCX$PWIPDRIVER.STB | Global symbol definitions for UCX$PWIPDRIVER.EXE
   SYS$COMMON:[SYSMGR]UCX$PWIP_SHUTDOWN.COM | PATHWORKS IP driver shutdown
   SYS$COMMON:[SYSMGR]UCX$PWIP_STARTUP.COM | PATHWORKS IP driver startup
   SYS$COMMON:[SYSEXE]UCX$PWIPSHUT.EXE | PATHWORKS IP driver shutdown
   SYS$COMMON:[SYSEXE]UCX$PWIPSYM.STB | Global symbol definitions for UCX$PWIPSYM.EXE

   Previous | Next | Contents